

**Mini Washbrook**



Wall Hung Urinal

VF-6401

**FEATURE**

Easy to Clean

Overflow hole

**SPECIFICATIONS**

Flush Valve Drillings: Single

Basin Dimensions: W320xL345xH605mm.

Material : Vitreous China

**COLOR AVAILABILITY**

White (WT)

**INCLUDED COMPONENTS**

 Wall fixing set for Lavatory

 Installation manual

Outlet rubber connector

Hanger for Urinal

**DIMENSIONAL DRAWING**

**SHIPPING WEIGHT**

Net Weight: 19 KG

Gross Weight: 22 KG



**STANDARDS CRITERIA**

TIS Standard

EN Standard

ASME Standards

This document is the property of American Standard. It can neither be reproduced, nor communicated, without authorization.

American Standard reserves the right to change dimensions and specifications without notice, we assume no liability for the use of obsolete dimensions.